**Proposed new light fittings in the Trinity Aisle**

Following consultation with the diocese it was suggested we consider alternative light fittings for the Trinity Aisle which are more in keeping with the existing fittings.

Following consultation with Andrews Electrical (architects consultation was not forthcoming) the suggested fittings are detailed below.

These fittings would be height – 9.8cm and width 14.6cm.

There would be two fittings, one each side of the Trinity Aisle at the same height and location as the existing fittings which are shown below.

A stone arch with a light on top

AI-generated content may be incorrect.

Existing fitting

Existing fittingA stone wall with windows

AI-generated content may be incorrect.

fitting

The suggested new fittings x2 and will be in the same location are shown below

A black light fixture with two lights

AI-generated content may be incorrect.