A kitchen with a sink and a paper towel dispenser

Description automatically generated

Kitchen area. Wiring and switches to be retained in current locations

Switch above the sink to be moved to the other side of the water heater or protected with a separate RCD as electrical contractor advises